LT800C
Grid-Connected Pipeline
· Hose Construction
· Inner Tube:EPDM rubber cured with peroxide
· Reinforcement:Multi-layer high-strength fiber braiding reinforced with spiralsteel wire
· Outer Layer:Corrugated black synthetic rubber(UL94VO flame-retardant)
· Temperature Range:-40℃~+93℃(-40°F~+200°F)
· Color:black
· Application:Suitable for conveyingfluid media such as air,water,water-glycol, oil-water emulsion, antifreeze fluid,phosphate esterhydraulicoil,etc.
	[bookmark: _GoBack]Size
	I.D
	O.D
	W.P
	B.R
	Vac.
	W.T

	 DASH
	in
	mm
	in
	mm
	PSI
	Mpa
	mm
	in Hg
	KG/M

	-12 
	3/4"
	19.1 
	1.15 
	29.1 
	150 
	1.03 
	19.1 
	29 
	0.501 

	-16 
	1"
	25.4 
	1.39 
	35.4 
	150 
	1.03 
	25.4 
	29 
	0.630 

	-20 
	11/4"
	31.8 
	1.65 
	419
	150 
	1.03 
	31.8 
	29 
	0.793 

	-24 
	11/2"
	38.1 
	1.90 
	48.2 
	150 
	103
	38.1 
	29 
	0.923 

	-32 
	2"
	50.8 
	2.44 
	61.9 
	150 
	1.03 
	50.8 
	29 
	1.266 

	-40 
	21/2"
	63.5 
	3.00 
	76.3 
	150 
	1.03 
	63.5 
	29 
	1.859 

	-48 
	3"
	76.2 
	3.50 
	89.0 
	150 
	1.03 
	76.2 
	29 
	2.213 

	-64 
	4"
	1,016
	4.53 
	115.1 
	150 
	1.03 
	1,016
	29 
	3.142 


The items marked with * are for reference only; the actual specifications are subject to the pipe body.
LT800B
Grid-Connected Pipeline
· Hose Construction
· Inner Tube:EPDM rubber cured with peroxide
· Reinforcement:One-layer high-strength fiber braiding reinforced
· OuterLayer:black synthetic rubber(UL94VO flame-retardant)
· Temperature Range:-40℃~+99℃(-40°F~+210°F)
· Color:black
· Application:Suitable for conveying fluid media such as air,water,water-glycol,oil-water emulsion, antifreeze fluid,phosphate esterhydraulic oil,etc.
	Size
	I.D
	O.D
	W.P
	B.R
	W.T

	DASH
	in
	mm
	in
	mm
	PSI
	Mpa
	mm
	KG/M

	-16 
	1"
	25.4 
	1.47 
	37.3 
	200 
	1.38 
	127.0 
	0.73 

	-24 
	11/2"
	38.1 
	2.08 
	52.8 
	200 
	1.38 
	203.2 
	1.31 

	-32 
	2"
	50.8 
	2.52 
	64.0 
	200 
	1.38 
	304.8 
	1.40 


The items marked with * are for reference only; the actual specifications are subject to the pipe body.
LT800A
LCP-Water Manifold Jumper Hose
· Hose Construction
· Inner Tube:EPDM rubber cured with peroxide
· Reinforcement:One layers of braided synthetic fiber
· Outer Cover:Black weather-resistant, ozone-resistant, UL94V0 flame-retardant special synthetic rubber
· Temperature Range:-40°C~+120°C (-40°F~+248°F)
· Color:red、black、blue
· Application:Suitable for medium fluids such as air, water, water glycol, oil-water emulsion, antifreeze, phosphate ester hydraulic oil, etc.
	Size
	
I.D
	
0.D
	
Max.W.P
	
Min.B.P
	
Min.B.R
	
W.T

	DASH
	IN
	mm
	mm
	MPa
	MPa
	mm
	kg/m

	-4 
	1/4
	6.4 
	12.1 
	1 
	4 
	25.4 
	0.13 

	-5 
	5/16
	7.7 
	14.5 
	1 
	4 
	31.5 
	0.18 

	-6 
	3/8
	9.5 
	15.9 
	1 
	4 
	38.1 
	0.19 

	-8 
	1/2
	12.7 
	19.8 
	1 
	4 
	69.9 
	0.25 

	-10 
	5/8
	15.9 
	23.1 
	7 
	4 
	88.9 
	0.30 

	-12 
	3/4
	19.1 
	26.2 
	1 
	4 
	114.3 
	0.35 

	-16 
	1 
	25.4 
	32.6 
	0.7 
	2.8 
	152.4 
	0.52 

	-20 
	1 1/4
	31.8 
	43 
	0.7 
	2.8 
	195 
	0.70 


The items marked with * are for reference only; the actual specifications are subject to the pipe body.
LT781
SAE 100R3 Fiber Braid Hose
· Hose Construction
· Inner Tube:blackoil resistant synthetic rubber
· Reinforcement:two braids of textile
· Outer Layer:black oil,weather,and abrasion resistant synthetic rubber
· Temperature Range:-40°C ~ +100°C (-40°F ~ +212°F)
· Application:Suitable to convey medium like petroleum based hydraulic oil,lubrication oil,water,and air.
	SIZE
(Dash)
	SIZE
(in.)
	  I.D.
(mm)
	O.D.
(mm)
	Max.W.P.
	Min.B.P.
	Min.B.R.
	W.T

	
	
	Min
	Max
	Min
	Max
	(MPa)
	(MPa)
	(mm)
	kg/m
	1bft

	-3
	3/16
	4.6
	5.5
	11.9
	13.6
	10.5
	42
	75
	0.15
	0.14

	-4
	1/4
	6.1
	7.0
	13.4
	15.1
	8.7
	34.8
	75
	0.16
	0.16

	-5
	5/16
	7.4
	8.5
	16.7
	18.3
	8.4
	33.6
	100
	0 .25
	0.21

	-6
	3/8
	9.3
	10.1
	18.3
	19.8
	7.8
	31.2
	100
	0.31
	0.26

	-8
	1/2
	12.3
	13.5
	22.8
	24.6
	7
	28
	125
	0.40
	0.38

	-10
	5/8
	15.5
	16.7
	26.2
	27.8
	6.1
	24.4
	140
	0.51
	0.42

	-12
	3/4
	18.5
	19.8
	30.7
	32.5
	5.2
	20.8
	150
	0.61
	0.58

	-16
	1
	25.1
	26.2
	36.8
	39.2
	3.9
	15.6
	205
	0.91
	0.74

	-20
	1 1/4
	31.4
	32.9
	42.8
	45.2
	2.6
	10.4
	250
	1.10
	0.77


The items marked with * are for reference only; the actual specifications are subject to the hose body.
LT782
SAE 100R4 Hydraulic Suction And Return Line
· Hose Construction
· Inner Tube:black oil resistant synthetic rubber
· Reinforcement:one or two braids of textile and a helical spiral-wire
· Outer Layer:black oil,weather,and abrasion resistant synthetic rubber
· Temperature Range:-40°C ~ +100°C (-40°F ~ +212°F)
· Application:Suitable to convey medium like petroleum based hydraulic oil,lubrication oil,water,and air.
	 SIZE
	 I.D
mm
	O.D
mm
	 Max.W.P
	 P.P
	 Min.B.P
	 W.T

	DASH
	IN
	Min
	Max
	Max
	MPa
	psi
	MPa
	psi
	MPa
	psi
	kg/m

	-12
	3/4
	18.2
	19.8
	34.0
	2.1
	305
	4.2
	610
	8.4
	1210
	0.68

	-16
	1
	24.6
	26.2
	40.0
	1.7
	250
	3.5
	510
	7
	1015
	0.84

	-20
	11/4
	30.6
	33.0
	48.0
	1.4
	200
	2.8
	410
	5.6
	810
	1.13

	-24
	11/2
	36.9
	39.3
	54.0
	1.05
	150
	2.1
	305
	4.2
	610
	1.41

	-32
	2
	49.2
	52.4
	68.0
	0.7
	100
	1.4
	200
	2.8
	410
	1.85

	-40
	21/2
	61.9
	65.1
	81.0
	0.4
	60
	0.85
	120
	1.7
	250
	2.28

	-48
	3
	74.6
	77.8
	93.0
	0.4
	60
	0.8
	120
	1.6
	230
	2.64

	-56
	31/2
	87.3
	90.5
	106.0
	0.3
	40
	0.6
	90
	1.25
	180
	3.02

	-64
	4
	100.0
	103.2
	120.0
	0.25
	40
	0.6
	70
	1
	145
	3.21


The items marked with * are for reference only; the actual specifications are subject to the hose body.
LT783
SAE 100R5 Hydraulic Hose
· Inner Tube:black oil resistant synthetic rubber
· Reinforcement:one braid of high tensile steel wire
· Outer Layer:textile braid impregnated with synthetic rubber
· Temperature Range:-40℃to+135℃(-40°F to 275°F),except air(not to exceed +93℃)and water(not to exceed+100℃)
· Application:Suitable for conveying medium like petroleum based hydraulicoil,lubrication oil,water,and air.
	SIZE
(Dash)
	SIZE
(mm)
	I.D. (mm)
	O.D. (mm)
	Max.W.P.
	Min.B.P.
	P.P
	Min.B.R.*
	W.T

	
	
	Min
	Max
	Min
	Max
	(MPa)
	(MPa)
	(MPa)
	(mm)
	kg/m

	-4
	5
	4.8
	5.5
	12.5
	13.7
	21
	84
	42
	75
	0.20

	-5
	6.3
	6.4
	7.2
	14.1
	15.3
	21
	84
	42
	85
	0.26

	-6
	8
	7.9
	8.7
	16.2
	17.6
	15.7
	62.8
	31.4
	100
	0.32

	-8
	11
	10.3
	11.1
	18.4
	20.0
	14
	56
	28
	115
	0.37

	-10
	12.5
	12.7
	13.7
	22.2
	24.0
	12.2
	48.8
	24.4
	140
	0.51

	-12
	16
	15.9
	17.0
	26.2
	28.0
	10.5
	42
	21
	165
	0.65

	-16
	22
	22.2
	23.3
	30.0
	32.2
	5.6
	22.4
	11.2
	185
	0.69

	-20
	29
	28.6
	29.8
	36.3
	38.9
	4.3
	17.2
	8.6
	230
	0.85

	-24
	35
	34.9
	36.1
	42.8
	45.2
	3.5
	14.0
	7
	265
	1.04

	-32
	46
	46.0
	47.2
	54.3
	57.6
	2.4
	9.6
	4.8
	335
	1.46

	-40
	60
	60.3
	61.9
	70.8
	74.2
	2.4
	9.6
	4.8
	610
	2.10

	-48
	76
	76.2
	77.8
	88.3
	91.7
	1.4
	5.6
	2.8
	840
	2.86


The items marked with * are for reference only; the actual specifications are subject to the hose body.
LT784
SAE 100R6 Fiber Braid Hose
· Hose Construction
· Inner Tube:Black oil-resistant synthetic rubber
· Reinforcement:One braid of textile
· Outer Layer:Black oil, weather,and abrasion resistant synthetic rubber
· Temperature Range:-40°C ~ +100°C (-40°F ~ +212°F)
· Application:Suitable for conveying medium like petroleum based hydraulic oil, lubrication oil,water,and air
	SIZE
	I.D.
mm
	O.D.
mm
	Max.W.P.
	Min.B.P.
	Min.B.R.
	W.T

	DASH
	IN
	Min
	Max
	Min
	Max
	MPa
	psi
	MPa
	psi
	mm
	kg/m

	-3
	3/16
	4.6
	5.5
	11.0
	12.2
	3.4
	500
	13.6
	2000
	50
	0.10

	-4
	1/4
	6.1
	6.9
	12.4
	13.6
	2.8
	400
	11.2
	1600
	65
	0.13

	-5
	5/16
	7.4
	8.5
	14.2
	15.4
	2.8
	400
	11.2
	1600
	80
	0.16

	-6
	3/8
	9.3
	10.1
	15.7
	16.9
	2.8
	400
	11.2
	1600
	80
	0.18

	-8
	1/2
	12.3
	13.5
	19.5
	21.1
	2.8
	400
	11.2
	1600
	100
	0.25

	-10
	5/8
	15.5
	16.7
	22.7
	24.3
	2.4
	340
	9.6
	1360
	125
	0.29

	-12
	3/4
	18.2
	19.8
	26.2
	27.8
	2.1
	340
	8.4
	1200
	150
	0.37


Note: The actual parameters are subject to the final atlas
LT785
GB1186 Compressed Air Hose
· Hose Construction
· Inner Tube:Black synthetic rubber
· Reinforcement:One or two braids of textile
· Outer Layer:Weather and abrasion resistant synthetic rubber
· Temperature Range:-40°C ~ +70°C (-40°F ~ +158°F)
· Application:Suitable to all kinds of power machinery and pneumatic tools to convey compressed air water or noble gases under the normal temperature
	SIZE
	I.D
mm
	O.D
mm
	Max.W.P
	Min.B.P
	W.T

	DASH
	IN
	Min
	Max
	Min
	MPa
	MPa
	Kg/m

	-8
	1/2
	12.5
	14.0
	23
	1.0
	4.0
	0.34

	-10
	5/8
	15.5
	17.0
	26
	1.0
	4.0
	0.40

	-12
	3/4
	18.5
	20.0
	29
	1.0
	4.0
	0.45

	-16
	1
	24.5
	26.0
	35
	1.0
	4.0
	0.48

	-20
	11/4
	31.5
	33.0
	45
	1.0
	4.0
	0.95

	-24
	11/2
	37.5
	39.0
	52
	1.0
	4.0
	1.25

	-32
	2
	50.0
	52.5
	66
	1.0
	4.0
	1.60

	-8
	1/2
	12.5
	14.0
	23
	2.0
	8.0
	0.34

	-10
	5/8
	15.5
	17.0
	26
	2.0
	8.0
	0.41

	-12
	3/4
	18.5
	20.0
	29
	2.0
	8.0
	0.46

	-16
	1
	24.5
	26.0
	35
	2.0
	8.0
	0.50

	-20
	11/4
	31.5
	33.0
	45
	2.0
	8.0
	0.97

	-24
	11/2
	37.5
	39.0
	52
	2.0
	8.0
	1.27

	-32
	2
	50.0
	52.5
	66
	2.0
	8.0
	1.70


Note: The actual parameters are subject to the final atlas
LT787
EN854 2TE&3TE Oil Return Line
· Hose Construction
· Inner Tube:Black oil resistant synthetic rubber
· Reinforcement:One or two braids of textile
· Outer Layer:Black oil,weather,and abrasion resistant synthetic rubber
· Temperature Range:-40°C ~ +100°C (-40°F ~ +212°F)
· Application:Suitable to convey petroleum-based hydraulic oil,crude oil,fuel oil, lubricating oil,emulsified oil, air,and water
	SIZE
	I.D.
mm
	O.D.
mm
	Max.W.P.
	P.P
	Min.B.P.
	Min.B.R.
	W.T

	DASH
	IN
	Min
	Max
	Min
	Max
	MPa
	MPa
	MPa
	mm
	kg/m

	-4
	1/4-1
	6.1
	6.9
	12.4
	13.6
	7.5
	15
	30
	40
	0.14

	-5
	5/16-1
	7.4
	8.5
	14.2
	15.4
	6.8
	13.6
	27.2
	50
	0.16

	-6
	3/8-1
	9.3
	10.1
	16.0
	17.2
	6.3
	12.6
	25.2
	60
	0.18

	-8
	1/2-1
	12.3
	13.5
	18.9
	20.5
	5.8
	11.6
	23.2
	70
	0.22

	-10
	5/8-1
	15.5
	16.7
	23.0
	24.6
	5.0
	10
	20.0
	90
	0.30

	-12
	3/4-1
	18.5
	19.8
	26.4
	28.0
	4.5
	9
	18.0
	110
	0.33

	-16
	1-1
	24.6
	26.2
	33.3
	35.7
	4.0
	8
	16.0
	130
	0.46

	-20
	1 1/4-1
	30.8
	32.8
	40.8
	43.2
	3.5
	7
	14.0
	140
	0.22

	-24
	1/4-2
	6.1
	6.9
	13.9
	15.1
	14.5
	29
	58
	45
	0.19

	-32
	5/16-2
	7.4
	8.5
	16.2
	17.4
	13.0
	26
	52
	55
	0.23

	-6
	3/8-2
	9.3
	10.1
	17.9
	19.1
	11.0
	22
	44.4
	70
	0.26

	-8
	1/2-2
	12.3
	13.5
	21.0
	22.6
	9.3
	18.6
	37.2
	85
	0.30

	-10
	5/8-2
	15.5
	16.7
	25.4
	27.0
	8.0
	16
	32.0
	105
	0.41

	-12
	3/4-2
	18.2
	19.8
	28.2
	29.8
	7.0
	14
	28.0
	130
	0.47

	-16
	1-2
	24.6
	26.2
	35.3
	37.7
	5.5
	11
	22.0
	150
	0.69

	-20
	1 1/4-2
	30.8
	32.8
	40.8
	43.2
	4.5
	9
	18.0
	190
	0.73

	-24
	1 1/2-2
	37.1
	39.1
	47.8
	50.2
	4.0
	8
	16.0
	240
	0.87

	-32
	2-2
	50.0
	52.0
	60.8
	64.0
	3.0
	6
	13.2
	300
	1.16


Note: The actual parameters are subject to the final atlas
LT788
Sand Blastlng Hose
· Hose Construction
· Inner Tube:Black abrasion resistant synthetic rubber (UPE layer is available)
· Reinforcement:Braided fiber or steel wire
· Outer Layer:Black weather and abrasion resistant synthetic rubber
· Temperature Range:-40℃~+70℃(-40°F~+158°F)
· Application:Apply to industries like railway,shipbuilding,and construction to remove rust on the metal surface
	SIZE
	I.D
mm
	O.D
mm
	Max.W.P
	P.P
	Min.B.P
	Min.B.R
	W.T

	DASH
	IN
	Min
	Max
	Min
	Max
	Min
	MPa
	MPa
	mm
	kg/m

	-10
	5/8
	15.5
	16.7
	28.2
	29.8
	1.0
	2.0
	4.0
	105
	0.98

	-12
	3/4
	18.8
	19.8
	34.2
	35.8
	1.0
	2.0
	4.0
	130
	1.14

	-16
	1
	24.8
	25.8
	42.8
	45.2
	1.0
	2.0
	4.0
	150
	1.50

	-20
	1 1/4
	31.6
	32.6
	48.8
	51.5
	1.0
	2.0
	4.0
	190
	1.80

	-24
	1 1/2
	37.7
	38.8
	57.5
	60.5
	1.0
	2.0
	4.0
	240
	2.10

	-28
	1 3/4
	44.6
	45.6
	62.5
	65.5
	1.0
	2.0
	4.0
	260
	2.30

	-32
	2
	50.7
	52
	69.5
	72.5
	1.0
	2.0
	4.0
	300
	2.75

	-40
	2 1/2
	63.7
	65.3
	83.5
	86.5
	0.8
	1.6
	3.2
	800
	3.50

	-48
	3
	75.5
	77.3
	100.0
	104.0
	0.8
	1.6
	3.2
	920
	4.50

	-56
	3 1/2
	88.5
	90.5
	113.0
	117.0
	0.8
	1.6
	3.2
	1100
	5.50

	-64
	4
	101.5
	104
	126.0
	130.0
	0.8
	1.6
	3.2
	1300
	6.50


Note: The actual parameters are subject to the final atlas
LT780
Oil Return Rubber Hose
· Hose Construction
· Inner Tube:Black oil resistant synthetic rubber
· Reinforcement:One braid or one spiral of textile
· Outer Layer:Black oil weather,and abrasion resistant synthetic rubber
· Temperature Range:-40°C ~ +100°C (-40°F ~ +212°F)
· Application:Suitable to convey petroleum-based hydraulic oil, lubricating oil,water,and air
	SIZE
	I.D
mm
	O.D
mm
	Max.W.P
	Min.B.P
	Min.B.R
	W.T

	DASH
	IN
	Min
	Max
	Min 
	Max
	MPa
	MPa
	mm
	Kg/m

	-4
	1/4"
	6.3
	6.9
	12.4
	13.6
	2
	8
	65
	0.138

	-5
	5/16"
	7.8
	8.5
	14.8
	16.0
	2
	8
	80
	0.18

	-6
	3/8"
	9.5
	10.8
	16.4
	17.6
	2
	8
	80
	0.189

	-8
	1/2"
	12.5
	13.8
	21.7
	23.3
	2
	8
	100
	0.339

	-10
	5/8"
	15.8
	16.6
	25.7
	27.3
	2
	8
	125
	0.443

	-12
	3/4"
	18.8
	19.8
	28.9
	30.5
	2
	8
	150
	0.528

	-14
	7/8"
	21.8
	22.8
	31.2
	32.8
	2
	8
	170
	0.535

	-16
	1"
	25.2
	26.2
	34.4
	36.0
	2
	8
	200
	0.59

	-20
	1-1/4"
	31.8
	32.8
	43.8
	46.2
	2
	8
	250
	0.954

	-24
	1-1/2"
	37.8
	38.8
	50.8
	53.2
	2
	8
	300
	1.189

	-32
	2"
	50.8
	52.2
	64.3
	66.7
	2
	8
	360
	1.612

	-40
	2-1/2"
	63.8
	65.5
	78.8
	81.2
	2
	6
	430
	2.272

	-48
	3"
	75.8
	77.5
	90.8
	93.2
	2
	6
	500
	2.693


Note: The actual parameters are subject to the final atlas

