LT1306
GB/T 27571 UPE Super Abrasion Resistant Concrete Hose
· Application:Apply to construction machinery like pump truck to delivery concretes.Its service life is several times more than average products in the market,and the high saturation characteristic of UPE means that this product will not react with the alkaline substance in the concrete.
· Hose Construction
· Inner Tube:UPE and NR&SBR synthetic rubber
· Reinforcement:2~4 plies of sprial steel cord
· Outer Layer:black NR&SBR synthetic rubber(UPE layer is available)
· Temperature Range:-30°C~+82°C (-22°F~+180°F)
· *The hose dimension,pressure and color can be customized based on the requirements.
	I.D
	0.D
	W.P
	Min.B.P
	Min.B.R
	W.T

	in
	mm
	in
	mm
	psi
	psi
	mm
	kg/m

	2
	51
	2.80
	71
	1250
	3750
	450
	2.85

	2.5
	64
	3.35
	85
	1250
	3750
	550
	3.70

	3
	76
	3.62
	103
	1250
	3750
	620
	5.25

	3.15
	80
	4.25
	108
	1250
	3750
	650
	6.03

	3.5
	89
	4.53
	115
	1250
	3750
	700
	6.83

	5
	127
	6.30
	160
	1250
	3750
	1050
	11.00


LT1305
HG/T 2192 Bulk Materials Suction & Discharge Hose
· [bookmark: _GoBack]Application:widely apply to large-scale projects like mining & construction, tunnel project and construction machinery like shield machine and slotter etc. Depending on its features of super abrasion and corrosion resistant,this product also suitable to transfer pulverized coal, cement, and various corrosive chemicals.
· Hose Construction
· Inner Tube:black,abrasionresistant, antistatic NR&SBRsynthetic rubber or UPE
· Reinforcement:Multi-spiral high tensile synthetic fibersand helix spiral-wire
· Outer Layer:NR&SBR or EPDM synthetic rubber
· Temperature Range:-30°C~+82°C (-22°F~+180°F)
· *The hose dimension, pressure and color can be customizedbased on the requirements.
	I.D
	O.D
	W.P
	Min.B.P
	Min.B.R
	W.T

	in
	mm
	in
	mm
	psi
	psi
	mm
	kg/m

	2
	51
	2.48
	63
	300
	750
	400
	1.55

	3
	76
	3.62
	92
	300
	750
	570
	2.60

	4
	102
	4.76
	120
	300
	750
	750
	4.50

	5
	127
	5.98
	152
	300
	750
	1000
	6.50

	6
	152
	7.76
	197
	300
	750
	1260
	19.5


LT1402
Furnace Cooling Water Delivery Hose
· Application::Big diameter flexible hose specially designed for cooling water conveyin steel mills, glass plans and foundries with high cooling efficiency and long service life, suitable for high-temp and hot metal or glass splashing environment.
· Hose Construction
· Inner Tube:Black EPDM synthetic rubber
· Reinforcement:Multi-spiral high tensile synthetic fibers and insulated spiral PP wire or helix spiral-wire
· Outer Layer:Black NBR&PVC fire retardant mixed rubber/thermal protective-layer and stainless steel armour
· Temperature Range:-40°C~+100°C(-40°F~+212°F);The cover radiant heat:540°C (1004°F)
· *The hose dimension, pressure and color can be customizedbased on the requirements.
	I.D
	O.D
	W.P
	Min.B.P
	Min.B.R
	W.T

	in
	mm
	in
	mm
	psi
	psi
	mm
	kg/m

	2
	51
	3.03
	77
	300
	750
	420
	1.85

	3
	76
	4.06
	103
	300
	750
	590
	2.90

	4
	102
	5.20
	132
	300
	750
	770
	5.30

	5
	127
	5.87
	149
	300
	750
	950
	6.45

	6
	152
	6.81
	173
	300
	750
	1160
	7.00

	8
	203
	9.17
	233
	300
	750
	1400
	15.00

	10
	254
	11.30
	287
	300
	750
	1700
	20.00



