LT305
17K Jumper Hose
· Inner Tube:UPE or PTFE (thickness 4.0mm)
· Reinforcement:Synthetic rubber, polyester fiber braiding and high-strength ultra-flexible copper-coated steel wire
· [bookmark: _GoBack]Outer Cover:Wear-resistant weather-resistant synthetic rubber + stainless steel armor
· Temperature Range:-30°C~+100°C (-22°F~+212°F)
· Compliance Standard:API 17K Third Edition
· Application:Features high pressure, lightweight, and long life characteristics, with superior corrosion resistance compared to traditional steel hose, can replace steel hose for deep-sea oil and gas transportation.
	I.D. (in)
	O.D. (mm)
	O.D. (mm)
	W.P.(Bar)
	T.P.
(Bar)
	
B.P.(Bar)
	Min.B.R.（m）
	Weight per meter of the hose in seawater.（kg/m）
	hose length（m）

	3
	76
	130
	232
	348
	580
	1.2
	4
	77

	8
	203
	275
	93
	139.5
	232.5
	2.1
	3
	77

	12
	304
	375
	18
	27
	45
	2.8
	108
	77

	16
	406
	485
	50
	75
	125
	3.2
	200
	77


LT301 F
Super Abrasion Resistant Frac Hose
· Hose Construction
· Inner Tube:UPE and synthetic rubber
· Reinforcement:multi-spiraled high tensile super flexible steel wire
· Outer Layer:abrasion and weather resistant synthetic rubber
· Temperature Range:-29°C~+100°C (-20°F~+212°F)
· Connector:intgral union,integral flange,or other connector types
· Application:Flexible line using for delivery water-based,oil-based,acid-based and foam fracturing fluids under high pressure in acid,sand and hydraulic fracturing works
	Size
	I.D.
	0.D.
	W.P.
	T.P.
	Min.B.R.
	W.T
	Volume
	Connector W.T
	Connection Type

	inch
	mm
	 mm
	Psi
	Psi
	m
	ft
	kg/m
	Ib/ft
	bbl/min
	m3/min
	kg
	Ib/set
	

	2"
	32 
	 81 
	15000 
	22500 
	1.2 
	3.94 
	11.5 
	7.7 
	4.5 
	0.72 
	25 
	55 
	2"FIG 1502 HammerUnion or
21/16"15K APIflange

	
	44 
	 95 
	15000 
	22500 
	1.4 
	4.59 
	18 
	12 
	9 
	1.46 
	45 
	99 
	3"FIG1502 Hammer Union or
31/16"15KAPlflange"

	
	51 
	107 
	15000 
	22500 
	1.4 
	4.59 
	20 
	13 
	12 
	1.91 
	59 
	130 
	

	2.5"
	58 
	122 
	15000 
	22500 
	1.5 
	4.92 
	24 
	16 
	15 
	2.39 
	61 
	134 
	

	
	64 
	126 
	15000 
	22500 
	1.5 
	4.92 
	27 
	18 
	18.5 
	2.90 
	75 
	165 
	

	3"
	69 
	135 
	15000 
	22500 
	1.6 
	5.25 
	30 
	20 
	21.5 
	3.42 
	91 
	201 
	

	
	76 
	145 
	15000 
	22500 
	1.6 
	5.25 
	35 
	24 
	26 
	4.13 
	102 
	225 
	

	4"
	89 
	164 
	15000 
	22500 
	2.0 
	6.56 
	52 
	35 
	36 
	5.72 
	132 
	291 
	4"FIG1502 Hammer Union or
41/16"15KAPlflange

	
	102 
	179 
	15000 
	22500 
	2.0 
	6.56 
	60 
	40 
	47 
	7.47 
	154 
	340 
	

	5"
	120 
	208 
	15000 
	22500 
	2.1 
	6.89 
	80 
	54 
	65 
	10.34 
	402 
	886 
	51/8"15KAPIflange

	
	127 
	216 
	15000 
	22500 
	2.1 
	6.89 
	86 
	58 
	73 
	11.61 
	407 
	897 
	

	5.5"
	140 
	243 
	15000 
	22500 
	2.2 
	7.22 
	110 
	74 
	88.5 
	14.07 
	653 
	1440 
	71/16"15KAPI flange

	6"
	152 
	255 
	15000 
	22500 
	2.3 
	7.54 
	125 
	84 
	104.5 
	16.62 
	703 
	1550 
	

	2"
	51 
	112 
	20000 
	30000 
	1.5 
	4.92 
	26 
	17 
	12 
	1.91 
	78 
	172 
	2"FIG 2002Hammer Union or
31/16"20KAPI flange

	2.5"
	64 
	133 
	20000 
	30000 
	1.6 
	5.25 
	36 
	24 
	18.5 
	2.90 
	103 
	227 
	3"FIG 2002Hammer Union or
31/16"20KAPlflange

	3"
	76 
	159 
	20000 
	30000 
	1.9 
	6.23 
	57 
	38 
	26 
	4.13 
	135 
	298 
	3"FIG 2002Hammer Union or
31/16"20KAPlflange

	4"
	102 
	202 
	20000 
	30000 
	2.1 
	6.89 
	94 
	63 
	47 
	7.47 
	400 
	882 
	41/16"20KAPI flange


Remark:According to the customer'srequriements,the I.D.of all the above sizes of hose assemblies can be made into full bore I.D.or non-full bore l.D.(A full bore hose assembly's effective flow I.D. is at least 95% of its nominal I.D.)The flow rate is calculated at a flow velocity of 50ft/s;LETONE recommends that the working flow velocity should not exceed 40ft/s.
LT304
Multi-Purpose Crude Oil Hose
· Hose Construction
· Inner Tube:Polymer composites
· Reinforcement:Multi-spiraled high tensile texile cords and highly flexible steel helix wire
· Outer Layer:Synthetic rubber
· Temperature Range:-40°C~+180°C (-40°F~+356°F)
· *The hose dimension, pressure and color can be customizedbased on the requirements.
· Application:The hose is suitable for delivering petroleum products such as fuel oil, crude oil, gasoline, etc. The hose inner layer is made of polymer composites, which makes the hose with strong corrosion resistance and high lubrication characteristics. Its excellent chemical stability prevents it from reacting with chemical substances in petroleum products,ensuring safe and efficient transportation of the medium.
	I.D.
	W.P
	Safety Factor

	in.
	mm
	MPa
	

	2
	51
	2-35
	2.5times

	2 1/2
	63
	2-35
	2.5times

	3
	76
	2-35
	2.5times

	3 1/2
	90
	2-35
	2.5times

	4
	102
	2-35
	2.5times

	5
	127
	2-35
	2.5times

	6
	152
	2-35
	2.5times


Note: Actual parameters are subject to the latest catalog. 
LT301 C
APISpec. 7K FSL0 |ABS High Pressure Cementing Hose
· Hose Construction
· Inner Tube:UPE and synthetic rubber or HNBR
· Reinforcement:Multi-spiraled high tensile super flexible steel wire
· Outer Layer:Abrasion and weather resistant synthetic rubber
· Temperature Range:-20°C~+121°C (-4°F~+250°F)
· Connector:Integral union or integral flange
· Application:Flexible connection in the manifold for delivery water-based and oil-based cement slurries under high pressure.
	Pressure Level
	I.D.
	O.D.
	W.P.
	P.P.
	Min.B.P.
	Min.B.R.
	Weight

	psi
	in.
	mm
	psi
	psi
	psi
	mm
	kg/m

	10000
	2
	83
	10000
	15000
	22500
	1000
	10.8

	
	2 1/2
	98
	10000
	15000
	22500
	1000
	19.4

	
	3
	129
	10000
	15000
	22500
	1400
	28

	
	3 1/2
	137
	10000
	15000
	22500
	1400
	33

	
	4
	154
	10000
	15000
	22500
	1600
	38.5

	
	5
	154
	10000
	15000
	22500
	1800
	56.5

	15000
	2
	101
	15000
	22500
	33750
	1200
	20.5

	
	3
	125
	15000
	22500
	33750
	1500
	36

	20000
	2
	106
	20000
	30000
	45000
	1500
	24

	
	3
	142
	20000
	30000
	45000
	1700
	44


Note: Actual parameters are subject to the latest catalog. 
LT301 D
API Spec. 7K-Rotary Drilling And Vibrator Hose
· Hose Construction
· Inner Tube:Synthetic rubber/HNBR/UPE/PTFE
· Reinforcement:Multi-spiraled high tensile super flexible steel wire
· Outer Layer:Abrasion and weather resistant synthetic rubber
· Temperature Range:-20°C~+121°C (-4°F~+250°F)
· Connector:Integral union, integral flange, or other connector types Full bore can be customized based on the requirements
· Full bore hose inner layer can be customized
· Application:Flexible connection between the upper end of the riser and the top drive/rotating assembly, and between the pump and the lower end of the riser in drilling, cementing, and well workover operations, for high-pressure mud pumping in oil drilling and exploration work
	Pressure Level
	I.D.
	O.D.
	W.P.
	P.P.
	Min.B.P.
	Min.B.R.
	Weight

	psi
	in.
	mm
	psi
	psi
	psi
	mm
	kg/m

	1500 Grade A
	2
	68
	1500
	2250
	3750
	800
	4.3

	
	2 1/2
	84
	1500
	2250
	3750
	800
	5.6

	2000 Grade B
	2
	68
	2000
	3000
	5000
	800
	4.3

	
	2 1/2
	84
	2000
	3000
	5000
	800
	5.6

	
	3
	97
	2000
	3000
	5000
	950
	6.5

	
	3 1/2
	113
	2000
	3000
	5000
	1000
	8.5

	
	4
	127
	2000
	3000
	5000
	1000
	10.4

	
	5
	157
	2000
	3000
	5000
	1200
	14.0

	
	6
	183
	2000
	3000
	5000
	1300
	18.0

	4000 Grade C
	2
	72
	4000
	6000
	10000
	800
	6.4

	
	2 1/2
	87
	4000
	6000
	10000
	800
	8.7

	
	3
	102
	4000
	6000
	10000
	1000
	11.1

	
	3 1/2
	119
	4000
	6000
	10000
	1200
	14.4

	
	4
	132
	4000
	6000
	10000
	1200
	16.0

	
	5
	162
	4000
	6000
	10000
	1400
	24.5

	
	6
	194
	4000
	6000
	10000
	1500
	33

	5000 Grade D
	2
	75
	5000
	7500
	12500
	800
	6.4

	
	2 1/2
	90
	5000
	7500
	12500
	800
	8.7

	
	3
	104
	5000
	7500
	12500
	1000
	11.1

	
	3 1/2
	121
	5000
	7500
	12500
	1200
	14.4

	
	4
	134
	5000
	7500
	12500
	1200
	16.0

	
	5
	167
	5000
	7500
	12500
	1400
	24.5

	
	6
	196
	5000
	7500
	12500
	1600
	33

	7500 Grade E
	2
	77
	7500
	11250
	18750
	900
	8.5

	
	2 1/2
	94
	7500
	11250
	18750
	1000
	10.5

	
	3
	110
	7500
	11250
	18750
	1000
	18.5

	
	3 1/2
	128
	7500
	11250
	18750
	1200
	20

	
	4
	150
	7500
	11250
	18750
	1400
	30

	
	5
	183
	7500
	11250
	18750
	1600
	49

	
	6
	212
	7500
	11250
	18750
	1600
	60


Note: Actual parameters are subject to the latest catalog. 
LT302
API 16C Series-Flexible Choke and Kill Line
· Hose Construction
· Inner Tube:HNBR/UPE
· Bore Type:Full bore
· Reinforcement:Multi-spiraled high tensile super flexible steel wire
· Outer Layer:High temperature and fire resistant synthetic rubber (resistant to 704°C open fire for 30 minutes)
· Outer Protection Layer:Stainless steel armor
· Temperature Range:-29°C~+121°C (-20°F~+250°F)
· Connector:Integral hammer union or integral flange
· Application:Flexible connection in the chock and kill manifolds for delivery oil-gas mixture that containing hydrogen sulfide (H2S) and other dangerous gases and various water-based, oil-based and foam killing fluids under high pressure.
	Pressure Level
	I.D.
	0.D.
	W.P.
	P.P.
	Min. B.P.
	Min.B.R.
	Weight

	psi
	in.
	mm
	psi
	psi
	psi
	mm
	kg/m

	5000
	2
	89
	5000
	7500
	11250
	1000
	9.5

	
	3
	115
	5000
	7500
	11250
	1200
	14.8

	
	3 1/2
	133
	5000
	7500
	11250
	1400
	20

	
	4
	147
	5000
	7500
	11250
	1600
	30

	10000
	2
	96
	10000
	15000
	22500
	1200
	15

	
	2 1/2
	126
	10000
	15000
	22500
	1600
	25

	
	3
	140
	10000
	15000
	22500
	1600
	33

	
	4
	167
	10000
	15000
	22500
	1800
	52

	15000
	2
	101
	15000
	22500
	33750
	1400
	21

	
	3
	141
	15000
	22500
	33750
	1600
	33

	
	4
	171
	15000
	22500
	33750
	2000
	56


Note: Actual parameters are subject to the latest catalog. 
LT303
API 16D Series-BOP Control Hose
· Hose Construction
· Inner Tube:NBR
· Tube Type:Full bore
· Reinforcement:4 plies of spiraled high tensile super flexible steel wire
· Outer Layer:High temperature and fire resistant synthetic rubber
· Protection Layer:Stainless steel armor
· Temperature Range:-40°C~+100°C (-40°F~+212°F) Fire resistance meets API Spec. 16D, 704°Cx5min
· Application:Hydraulic control line for remotely control the blowout preventer (BOP) at high pressure.
	I.D.
	W.P.
	P.P.
	Min. B.P.
	Min. B.R.
	Weight

	(in.)
	(psi)
	(psi)
	(psi)
	(mm)
	(kg/m)

	1/2
	5000
	7500
	15000
	300
	1.9

	3/4
	5000
	7500
	15000
	400
	2.7

	1
	5000
	7500
	15000
	500
	3.6

	1 1/2
	5000
	7500
	15000
	700
	5.3

	2
	5000
	7500
	15000
	800
	7.2


Note: Actual parameters are subject to the latest catalog. 

